**Anexa 10 c.**

***certificatul de Inspecţie Tehnică pentru:***

***• autovehicule cu masa maximă autorizată cuprinsă între 3,5 şi 6 tone***

***• remorca cu masa maximă autorizată care nu depăşeşte 3,5 tone***

*varianta în limba engleză*

**Certificate No: ….……….**

**ECMT Certificate of Roadworthiness Test for Motor Vehicles and Trailers[[1]](#footnote-1)**

|  |
| --- |
| Registration Number: |
| Certificate of Compliance Number: |
| Vehicle Type and Make:[[2]](#footnote-2) |
| Vehicle Identification Number (VIN): |
| Engine Type / Number:[[3]](#footnote-3) |

The

*[Name and address of the Company or Authority]*

Body or Establishment designated and directly supervised by the State of Registration for the purpose of UNECE Agreement of 1997, or of the UNECE Consolidated Resolution R.E.1 (TRANS/SC.1/294/Rev.5) as amended in 2001 (TRANS/WP.1/2001/25) or as subsequently amended, or of Directive 2009/40/EC as amended by Commission Directive 2010/48/EU or as subsequently amended,

hereby confirms that the said vehicle is in compliance with the provisions of the texts above, including at least the following items to be compulsory checked:

❑ Braking systems (including antiblocking systems, compatible with the trailer and vice‑versa)

❑ Steering wheel3 and steering devices

❑ Visibility

❑ Lamps, reflectors and electrical equipment

❑ Axles, wheels, tyres and suspension (including minimum tread depth of tyres)

❑ Chassis and chassis attachments (including rear and lateral protective devices)

❑ Other equipment, including:

❑ Warning triangle3

❑ Tachograph (presence of and integrity of seals)3

❑ Speed limitation device3

❑ Absorption coefficient.3,[[4]](#footnote-4)

Place Date Signature and stamp[[5]](#footnote-5)

Note: Next roadworthiness test required before:[[6]](#footnote-6)

1. . Semi-trailers included. [↑](#footnote-ref-1)
2. . Trailer type, if trailer. [↑](#footnote-ref-2)
3. . Not applicable to trailer. [↑](#footnote-ref-3)
4. . According to UNECE regulation R24.03 or as subsequently amended, or to Directive 72/306/EEC or as subsequently amended, or to Directive 2005/78/EC or as subsequently amended; for EURO VI and positive ignition engines not required. [↑](#footnote-ref-4)
5. . Certificate may be filled in, stamped and signed manually or electronically. [↑](#footnote-ref-5)
6. . 12 months after the date of the test, and at the latest before the end of this same month. [↑](#footnote-ref-6)